{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["userSTP0360"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"userSTP0360","index":0,"n_rows":63,"n_cols":36,"rows_kept":63,"flags":["formulas_cached_only"]}
["순서","조사년도","배출구\n일련번호","배출구명","허가증상\n배출구번호","배출구유형","배출구\n높이(m)","상부배출구\n내경(m)","측정공위치\n내경(m)","측정일자","자가측정방법","오염물질","농도","단위","배출허용기준","배출허용기준\n없음표시","배출가스유량\n(S㎥／min)","TMS 배출가스유량\n(S㎥/mon)","배출가스속도\n(m／s)","배출가스온도\n(℃)","수분량(％)","표준산소농도\n(％)"," 실측산소농도\n(％)","기상","기온(℃)","습도(％)","기압(mmHg)","풍향","풍속(m/s)","연료명및사용량","원료명및사용량","검사기기명","검사방법","검사기관명","환경기술인","환경기술인의견"]
[1,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","암모니아",7.2,"ppm","16","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[2,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","황화수소",0,"ppm","1.6","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[3,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","이황화탄소",0,"mg/S㎥","8","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[4,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","시안화수소",0.05,"mg/S㎥","3.2","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[5,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","페놀화합물(C6H5OH)",0,"mg/S㎥","3.2","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[6,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","포름알데히드",0,"ppm","4","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[7,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","아세트알데히드",0,"ppm","10","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[8,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","벤젠",0,"ppm","4.8","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[9,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","디클로로메탄",0,"ppm","40","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[10,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","트리클로로에틸렌 ",0,"ppm","40","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[11,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","1,3-부타디엔",0,"ppm","4.8","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[12,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","1,2-디클로로에탄 ",0,"ppm","12","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[13,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","테트라클로로에틸렌",0,"mg/S㎥","10","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[14,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","클로로포름",0,"ppm","5","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[15,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","아크릴로니트릴",0,"ppm","3","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[16,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","스틸렌",0,"ppm","23","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[17,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","에틸벤젠",0,"mg/S㎥","23","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[18,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","사염화탄소",0,"ppm","3","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[19,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","카드뮴화합물(Cd로서)",0,"ppm","0.016","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[20,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","납화합물(Pb로서)",0,"ppm","0.16","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[21,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","크롬화합물(Cr로서)",0,"ppm","0.16","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[22,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","구리 및 그 화합물",0,"ppm","3.2","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[23,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","아연화합물(Zn로서)",0.375,"mg/S㎥","3.2","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[24,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","니켈 및 그 화합물",0,"mg/S㎥","1.6","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[25,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","베릴륨 및 그 화합물",0,"ppm","0.05","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[26,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","비소화합물(As로서)",0,"ppm","0.16","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[27,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-13","대행의뢰","이황화메틸",0,"ppm","3","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[28,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-14","대행의뢰","브롬화합물",0,"ppm","2.4","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[29,"2025","1","굴뚝1","1","TMS부착배출구(원형)",62,0.9,0.9,"2025-03-14","대행의뢰","불소화합물(F로서)",0,"ppm","1.6","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[30,"2025","2025","2025","2025","2025","2025","2025","2025","2025-03-14","대행의뢰","수은화합물(Hg로서)",0,"ppm","0.04","  ",616.4,0,20.79,178.2,15.59,12,7.4,"흐림",1.1,"65","767","동","1.3",{"$nulls":5},"송정은"]
[31,"2025","2025","2025","2025","2025","2025","2025","2025","2025-03-20","대행의뢰","다환 방향족 탄화수소류",0,"ppm",0.05]
[32,"2025",{"$nulls":7},"2025-05-29",null,"카드뮴화합물(Cd로서)",0,"mg/S㎥","0.016"]
[33,"2025",{"$nulls":7},"2025-05-29",null,"시안화수소",0,"ppm","3.2"]
[34,"2025",{"$nulls":7},"2025-05-29",null,"납화합물(Pb로서)",0,"mg/S㎥","0.16"]
[35,"2025",{"$nulls":7},"2025-05-29",null,"크롬화합물(Cr로서)",0,"mg/S㎥","0.16"]
[36,"2025",{"$nulls":7},"2025-05-29",null,"비소화합물(As로서)",0,"ppm","0.16"]
[37,"2025",{"$nulls":7},"2025-05-29",null,"수은화합물(Hg로서)",0,"mg/S㎥","0.04"]
[38,"2025",{"$nulls":7},"2025-05-29",null,"불소화합물(F로서)",0,"ppm","1.6"]
[39,"2025",{"$nulls":7},"2025-05-29",null,"니켈 및 그 화합물",0,"mg/S㎥","1.6"]
[40,"2025",{"$nulls":7},"2025-05-29",null,"페놀화합물(C6H5OH)",0,"ppm","3.2"]
[41,"2025",{"$nulls":7},"2025-05-29",null,"베릴륨 및 그 화합물",0,"mg/S㎥","0.05"]
[42,"2025",{"$nulls":7},"2025-05-29",null,"벤젠",0,"ppm","4.8"]
[43,"2025",{"$nulls":7},"2025-05-29",null,"사염화탄소",0,"ppm","3"]
[44,"2025",{"$nulls":7},"2025-05-29",null,"이황화메틸",0.00073,"ppm","3"]
[45,"2025",{"$nulls":7},"2025-05-29",null,"클로로포름",0,"ppm","5"]
[46,"2025",{"$nulls":7},"2025-05-29",null,"포름알데히드",0,"ppm","4"]
[47,"2025",{"$nulls":7},"2025-05-29",null,"아세트알데히드",0,"ppm","10"]
[48,"2025",{"$nulls":7},"2025-05-29",null,"1,3-부타디엔",0,"ppm","4.8"]
[49,"2025",{"$nulls":7},"2025-05-29",null,"브롬화합물",0,"ppm","2.4"]
[50,"2025",{"$nulls":7},"2025-05-29",null,"아연화합물(Zn로서)",0,"mg/S㎥","3.2"]
[51,"2025",{"$nulls":7},"2025-05-29",null,"암모니아",4.8,"ppm","16"]
[52,"2025",{"$nulls":7},"2025-05-29",null,"황화수소",0,"ppm","1.6"]
[53,"2025",{"$nulls":7},"2025-05-29",null,"이황화탄소",0,"ppm","8"]
[54,"2025",{"$nulls":7},"2025-05-29",null,"스틸렌",0,"ppm","23"]
[55,"2025",{"$nulls":7},"2025-05-29",null,"구리 및 그 화합물",0,"mg/S㎥","3.2"]
[56,"2025",{"$nulls":7},"2025-05-29",null,"디클로로메탄",0,"ppm","40"]
[57,"2025",{"$nulls":7},"2025-05-29",null,"테트라클로로에틸렌",0,"ppm","10"]
[58,"2025",{"$nulls":7},"2025-05-29",null,"1,2-디클로로에탄 ",0,"ppm","12"]
[59,"2025",{"$nulls":7},"2025-05-29",null,"에틸벤젠",0,"ppm","23"]
[60,"2025",{"$nulls":7},"2025-05-29",null,"트리클로로에틸렌 ",0,"ppm","40"]
[61,"2025",{"$nulls":7},"2025-05-29",null,"아크릴로니트릴",0,"ppm","3"]
[62,"2025",{"$nulls":7},"2025-05-30",null,"다환 방향족 탄화수소류",0,"ng/㎥",0.05]